Task 3: Test the servo motor with different duty cycle values

Answer Q1 in Moodle: What are the minimum and maximum values effective duty cycle values of your motor?

Minimum value: 1.5%

Maximum value: 12%